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Electrician safety checklist
Trade-specific safety checks for electricians - run through before work starts, every time.
	Site address
	[Full site address]

	Date
	[Date]

	Checked by
	[Name]



Checks
	Check
	Yes
	No
	N/A

	Lock-out / tag-out - circuit isolated, locked off, key retained
	☐
	☐
	☐

	Test before touch - proven dead with calibrated test equipment
	☐
	☐
	☐

	RCD protection confirmed on circuits being worked on
	☐
	☐
	☐

	No live working unless no reasonable alternative and fully justified
	☐
	☐
	☐

	Ladders and access equipment inspected before use
	☐
	☐
	☐

	Fire risk - no overloaded temporary supplies; extinguishers accessible
	☐
	☐
	☐

	Asbestos awareness - work stops if suspect material is disturbed
	☐
	☐
	☐

	Working in lofts / confined spaces - lighting and access checked
	☐
	☐
	☐

	PPE worn - insulated tools, eye protection, dust mask where needed
	☐
	☐
	☐

	Site left safe - all circuits tested, covers replaced, area clean
	☐
	☐
	☐



Actions required
[List any issues found and what was done]
Sign-off
	Checked by
	Signature
	Date
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