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HVAC technician safety checklist
Trade-specific safety checks for hvac technicians - run through before work starts, every time.
	Site address
	[Full site address]

	Date
	[Date]

	Checked by
	[Name]



Checks
	Check
	Yes
	No
	N/A

	Refrigerant handling - F-gas certified personnel only; recovery machine available
	☐
	☐
	☐

	Electrical isolation - unit isolated and proven dead before opening panels
	☐
	☐
	☐

	Working at height - roof / ladder access risk-assessed; fall protection where needed
	☐
	☐
	☐

	Manual handling - outdoor units and cylinders moved with aids or assistance
	☐
	☐
	☐

	Pressure systems - gauges checked; no work on pressurised components without procedure
	☐
	☐
	☐

	Ventilation - no refrigerant release in confined spaces
	☐
	☐
	☐

	Hot surfaces - compressor and pipework allowed to cool before handling
	☐
	☐
	☐

	PPE worn - gloves and eye protection when handling refrigerant or brazing
	☐
	☐
	☐

	Brazing - hot works permit, fire extinguisher at hand, nitrogen purge used
	☐
	☐
	☐

	Site left safe - panels refitted, system tested, area clean
	☐
	☐
	☐



Actions required
[List any issues found and what was done]
Sign-off
	Checked by
	Signature
	Date
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