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Plasterer safety checklist
Trade-specific safety checks for plasterers - run through before work starts, every time.
	Site address
	[Full site address]

	Date
	[Date]

	Checked by
	[Name]



Checks
	Check
	Yes
	No
	N/A

	Dust - mask worn when mixing plaster; background ventilated
	☐
	☐
	☐

	Manual handling - 25kg bags lifted correctly; mixer positioned safely
	☐
	☐
	☐

	Working at height - hop-ups and platforms stable for ceiling work
	☐
	☐
	☐

	Slips - wet plaster spills cleaned; sheeting secured
	☐
	☐
	☐

	Eye protection - worn when mixing and when working overhead
	☐
	☐
	☐

	Skin - gloves or barrier cream; wash hands before eating
	☐
	☐
	☐

	Electrical safety - sockets masked, not painted over; power off if needed
	☐
	☐
	☐

	PPE worn - dust mask, eye protection, gloves as a minimum
	☐
	☐
	☐

	Site left safe - tools cleaned, buckets emptied, area swept
	☐
	☐
	☐

	Drying - customer advised on drying times before decorating
	☐
	☐
	☐



Actions required
[List any issues found and what was done]
Sign-off
	Checked by
	Signature
	Date
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