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Tiler tile care instructions
Leave-behind care guide for your customer - how to look after new tiling.
Job details
	Customer
	[Name]

	Address
	[Address]

	Areas tiled
	[e.g. bathroom walls and floor]

	Tile type
	[e.g. 600x300 ceramic]

	Grout used
	[Brand and colour]

	Sealant used
	[Brand, if any]

	Date completed
	[Date]



First 48 hours
[Do not walk on floor tiles for 24 hours. Do not get wall tiles wet for 48 hours while adhesive and grout cure.]
Cleaning
[Use a pH-neutral cleaner. Avoid bleach, acids and abrasive pads on grout and natural stone.]
Sealing
[Reseal natural stone every [12] months with [product]. Ceramic and porcelain do not need sealing.]
Maintenance
[Re-grout or re-seal silicone around baths and showers every [2–3] years or when it discolours.]
Sign-off
	Tiler
	Customer
	Date
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