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Tiler safety checklist
Trade-specific safety checks for tilers - run through before work starts, every time.
	Site address
	[Full site address]

	Date
	[Date]

	Checked by
	[Name]



Checks
	Check
	Yes
	No
	N/A

	Dust - mask worn when cutting tiles; wet cutting preferred
	☐
	☐
	☐

	Manual handling - tile boxes lifted with bent knees; no overloading
	☐
	☐
	☐

	Slips - wet floors signed and dried; spills cleaned immediately
	☐
	☐
	☐

	Eye protection - worn when cutting, drilling or mixing
	☐
	☐
	☐

	Knee protection - knee pads for floor work
	☐
	☐
	☐

	Electrical safety - power isolated where tiling near sockets or showers
	☐
	☐
	☐

	Sharp edges - cut tiles handled with gloves
	☐
	☐
	☐

	Ventilation - adequate airflow when using solvent-based adhesives
	☐
	☐
	☐

	PPE worn - eye protection, dust mask, knee pads, gloves as needed
	☐
	☐
	☐

	Site left safe - offcuts cleared, tools secured, area clean
	☐
	☐
	☐



Actions required
[List any issues found and what was done]
Sign-off
	Checked by
	Signature
	Date
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