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Landscaper safety checklist
Trade-specific safety checks for landscapers - run through before work starts, every time.
	Site address
	[Full site address]

	Date
	[Date]

	Checked by
	[Name]



Checks
	Check
	Yes
	No
	N/A

	Manual handling - turf rolls, soil bags and slabs lifted with aids or team lifts
	☐
	☐
	☐

	Power tools - guards in place; fuel stored safely away from work area
	☐
	☐
	☐

	Underground services - CAT scan before digging; hand-dig near services
	☐
	☐
	☐

	Working near roads - high-vis worn; materials not obstructing footpaths
	☐
	☐
	☐

	Pesticides and chemicals - COSHH sheets available; kept locked away from children/pets
	☐
	☐
	☐

	Sun and heat - water available; breaks in shade on hot days
	☐
	☐
	☐

	Slips and trips - muddy areas boarded; tools not left in walkways
	☐
	☐
	☐

	Noise - considerate hours; hearing protection for prolonged machine use
	☐
	☐
	☐

	PPE worn - steel-toe boots, gloves, eye protection as needed
	☐
	☐
	☐

	Site left safe - excavations fenced, tools secured, gates closed
	☐
	☐
	☐



Actions required
[List any issues found and what was done]
Sign-off
	Checked by
	Signature
	Date
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