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Plumber safety checklist
Trade-specific safety checks for plumbers - run through before work starts, every time.
	Site address
	[Full site address]

	Date
	[Date]

	Checked by
	[Name]



Checks
	Check
	Yes
	No
	N/A

	Water supply isolated and confirmed off before starting work
	☐
	☐
	☐

	Gas supply checked - no gas work undertaken unless Gas Safe registered
	☐
	☐
	☐

	Hot works permit in place where soldering or heat is used
	☐
	☐
	☐

	Adequate ventilation where flux, solvents or sealants are used
	☐
	☐
	☐

	Electrical safety - power isolated where working near wiring or immersion heaters
	☐
	☐
	☐

	Manual handling - heavy items (cylinders, baths, boilers) lifted with assistance or aids
	☐
	☐
	☐

	Slip protection - water spills cleaned immediately; warning signs where needed
	☐
	☐
	☐

	Legionella awareness - stagnant systems flushed before recommissioning
	☐
	☐
	☐

	PPE worn - eye protection when cutting, gloves when handling chemicals
	☐
	☐
	☐

	Site left safe - open pipework capped, tools removed, area clean
	☐
	☐
	☐



Actions required
[List any issues found and what was done]
Sign-off
	Checked by
	Signature
	Date
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