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Roofer safety checklist
Trade-specific safety checks for roofers - run through before work starts, every time.
	Site address
	[Full site address]

	Date
	[Date]

	Checked by
	[Name]



Checks
	Check
	Yes
	No
	N/A

	Working at height - edge protection or scaffold in place before access
	☐
	☐
	☐

	Fragile roofs - crawling boards used; no walking on unsupported areas
	☐
	☐
	☐

	Weather - work stops in high wind, ice, or heavy rain
	☐
	☐
	☐

	Falling objects - exclusion zone below; toe boards and debris netting
	☐
	☐
	☐

	Ladders - secured at top, correct angle, inspected before use
	☐
	☐
	☐

	Manual handling - tile bundles and lead rolls lifted with aids or assistance
	☐
	☐
	☐

	Overhead lines - minimum clearance checked where present
	☐
	☐
	☐

	Asbestos - old soffits, flues or cement sheets sampled before disturbance
	☐
	☐
	☐

	Hot works - permit for torch-on felt; extinguisher at hand
	☐
	☐
	☐

	PPE worn - harness where required, hard hat, gloves, safety boots
	☐
	☐
	☐



Actions required
[List any issues found and what was done]
Sign-off
	Checked by
	Signature
	Date
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